COMPRESSED AIR
· Follow manufacturer's general instructions and comply with legislated safety requirements.
· The equipment must be properly maintained according to the manufacturer’s requirements.
· Hoses must be checked on a regular basis for cuts, bulges, or other damage.  Ensure that defective hoses are repaired or replaced.
· All hose connectors must be of the quick disconnect pressure release type with a "safety chain/cable".
· A proper pressure regulator and relief device must be in the system to ensure that correct desired pressures are maintained.

· The correct air supply hoses must be used for the tool/equipment being used.

· Compressed air shall not be used to clean clothes, machinery, work benches or floors.
· Ensure the air pressure has been turned off and the line pressure relieved before disconnecting the hose or changing tools.

· Wear personal protective equipment such as eye protection and face shields and ensure other workers in the area are made aware of or have restricted access to the hazard area.
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