EXTENSION CORDS

· All portable extension cords must be of the outdoor type, rated for 300 volts, and have an insulated grounding conductor.

· All extension cords will be CSA approved and inspected before use.

· Defective cords must not be used.

· They must either be destroyed or be tagged and removed from the worksite until repaired.

· Extension cords must be protected during use to prevent damage from sharp edges, movement of materials, and flame cutting.

· All extension cords are to be placed in such a way that they will not be a tripping or falling hazard.

· All extension cords used in hazardous areas or in damp locations are to be protected by approved ground fault protection.

· All frayed, cut, or spliced extension cords are to be tagged and removed from service.
