LIGHT WELDING OPERATIONS

· Welding equipment should be inspected prior to use.

· Check cables for bare wires that can arc and cause shock and burn injuries. 

· Avoid welding directly over your body as molten metal may drip on to your body causing burns. 

· Use a fire blanket to reduce the risk of fires. 

· Have a fire extinguisher or water hose at hand before starting the welding.

· DO NOT weld where flammable liquid or gases are present.

· Wear personal protective equipment such as auto darkening welding shields, heat resistant gloves and fire-retardant clothing.

· Where using a manual or air operated chipping hammer to remove hardened flux and slag, wear the welding shield to prevent face and eye injuries.

· Use welding screens where other employees are present to prevent flashing of the eyes.

· Check the work area up to 1 hour after finishing the welding job to ensure that no fires have been started.
