PROPER MOUNTING / DISMOUNTING OF CONSTRUCTION EQUIPMENT


· Look before and where you step; 

· Use every available hand – hold; 

· Maintain 3-point contact; 

· Step squarely, never at an angle;

· Never attempt to mount / dismount from moving equipment; 

· Never jump off equipment;

· Broken or missing handholds and footholds are repaired or replaced immediately.

· Worn of slippery surfaces of the access route should be replaced with skid-resistant surfaces.  

· Operators should keep the cabs and access areas clean and tidy. 

· Running-boards, treads, steps, footholds and platforms must be kept clear of mud, ice, snow, grease and other hazards that can cause slips, trips or falls.

· It is recommended that loose or torn clothing be avoided where possible, as it may become caught on equipment or otherwise interfere with use of the access route.

· Caution, care and extra time must be used when mounting and dismounting from construction equipment during the winter.
