Daily Aerial Work Platform Inspection Checklist
Date: __________________ 	Operator: _______________	Vehicle #: __________________
Hour Meter: ____________	Fuel: __________________
	PRE START-UP WALK-AROUND
	PASS
	FAIL
	N/A
	POWERED CHECKS
	PASS
	FAIL
	N/A

	Wheels, tires, axels – condition/inflation
	
	
	
	Engine – starts/oil pressure
	
	
	

	Hydraulic Components
	
	
	
	Battery – charge level
	
	
	

	Data Plate
	
	
	
	Gauges & instruments – hour meter/warning lights
	
	
	

	Annual Inspection verified
	
	
	
	GROUND & PLATFORM CONTROLS
	PASS
	FAIL
	N/A

	Battery Tray
	
	
	
	Elevating section – raise/lower
	
	
	

	Cover Panels
	
	
	
	Drive – forward/reverse
	
	
	

	Engine – fluids/filters/belts/hoses
	
	
	
	Steer – left/right
	
	
	

	Batteries – clean/dry/secure/caps, etc. 
	
	
	
	Horn
	
	
	

	Fuel tank/level
	
	
	
	Outriggers/stabilizers
	
	
	

	Hydraulic oil level
	
	
	
	Pothole protection
	
	
	

	Lights/strobes
	
	
	
	Function-enable device
	
	
	

	Placards/labels/decals
	
	
	
	Manual lowering system
	
	
	

	Top of base – leaks/debris
	
	
	
	Safety interlocks
	
	
	

	Accessory plugs & cables
	
	
	
	WORKPLACE INSPECTION
	PASS
	FAIL
	N/A

	Elevating section – general condition
	
	
	
	Drop-offs/holes
	
	
	

	Hydraulic cylinders & pin locks
	
	
	
	Bumps & floor/ground obstacles
	
	
	

	Pivot Pins – wear/secured
	
	
	
	Debris
	
	
	

	Power track – lines/hoses
	
	
	
	Overhead obstacles
	
	
	

	Platform – guard rails/toe board/extension
	
	
	
	Energized power lines
	
	
	

	Weather-resistant storage compartment – appropriate manuals
	
	
	
	Hazardous locations
	
	
	

	All controls – clearly marked
	
	
	
	Ground surface/support conditions
	
	
	

	Other:
	
	
	
	Pedestrian/vehicle traffic
	
	
	

	
	
	
	
	Wind/weather conditions
	
	
	

	
	
	
	
	Other hazards:
	
	
	

	Comments/Deficiencies:

	

	

	

	Operator Name:
	Operator Signature:	
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