Scaffold Inspection Checklist
Date: 						Inspected By: 		                   		    
Location:  								                     		    
	Item #
	Scaffold Inspection Checklist
	Yes
	No
	N/A

	1
	Erection and inspection completed by a competent worker
	
	
	

	2
	Scaffold is erected with vertical members plumb and ledgers and bearers level
	
	
	

	3
	All scaffold components present, tight and secure
	
	
	

	4
	No tubes or members over extended and hazardous
	
	
	

	5
	Base plates and screws firmly supported on all legs and mudsills
	
	
	

	6
	Levelling adjustment screws extended more than the lesser of two-thirds of its total length or 60 centimetres
	
	
	

	7
	Effectively guyed or secured to a building or structure where the height of the scaffold exceeds 3 times its minimum base
	
	
	

	8
	Building ties or guys placed at a height not exceeding 3 times the scaffold minimum base dimensions, and at horizontal intervals of every third bay or 6.4m, whichever is lesser, at the end of the scaffold.
	
	
	

	9
	Rolling scaffold wheels are locked with outriggers extended to maintain a maximum height of 3 times the smallest base dimensions
	
	
	

	10
	Platform planks have cleats on underside at each end with wood/angle iron
	
	
	

	11
	Platform planks tied down securely
	
	
	

	12
	Platform planks maximum span 3.05m for light duty and 2.13m for heavy duty
	
	
	

	13
	Separate ladder(s) used for scaffold access
	
	
	

	14
	Ladder(s) securely fastened in place with siderails extending approximately one metre above the uppermost working level
	
	
	

	15
	Perimeter placed on work surfaces – toe boards permanent and temporary with dimensions of 2.54cm x 10.16cm
	
	
	

	16
	Safety cage around vertical ladders where a potential fall is more than 7.32 metres in length.
	
	
	

	17
	Open sides have guard rails with a top rail located 0.9 metres to 1.1 metres above the working surface and an intermediate rail located midway between the top rail and the working surface.
	
	
	

	18
	Separate rope or handline in place at all platforms to raise and lower tools or material
	
	
	

	19
	Warning devices/signs provided if erected over walkways or roadways 
	
	
	

	20
	Minimum clearance of 5.5 meters from overhead powerlines is maintained where there is no permit from appropriate utilities 
	
	
	

	21
	Scaffold constructed and maintained according to certified engineer or manufacturer’s’ specifications or drawings
	
	
	

	22
	Inspected daily by a competent worker, tagged at each entry and exit point
	
	
	



	Item #
	Corrective Action Required
	Assigned to
	Completion date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	Signature of Inspectors:
	1

	2.
	3.
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