	JOB SAFETY ANALYSIS (JSA)

	
Date:                                                                                       Location: ______________________________________________________

Job Being Performed:  Operation of an Aerial Work Platform


	Sequence of Events / Work Activity
	Potential Hazards
	Preventative / Control Measures

	Gather tools and equipment for task (including fall protection equipment)
	Awkward positioning causing strains or musculoskeletal injury (MSI)


	Use proper lifting mechanics (i.e. lift with legs) to gather tools needed for work in AWP. 

For heavier items, have a second worker aid with lifting. 


	Setting up AWP on the worksite
	Operator not appropriately trained or authorized to use AWP which could result in property damage, injury, or fatality
	Ensure that the anyone who is required to work from the AWP has current AWP training. 

Ensure that the operator is competent in operating the AWP.

Any workers working on the AWP are required to have a valid fall protection training certificate in accordance with the NL OHS legislation. 

Follow the company’s SWP for operation of an AWP.


	1. 
	PPE not available or inadequate. 
	Ensure workers have fall arrest equipment (harness and a lanyard) that is properly fitted. 

Ensure that workers are conducting inspections of their fall arrest equipment prior to operating the AWP. 

Ensure workers have other PPE deemed necessary based on the hazards present (hard hats, reflective vests, steel toed boots, safety glasses, hearing protection, respirators, etc.).  

Ensure workers have inspected their PPE prior to use. 

	2. 
	Uneven ground causing tip-overs
	Ensure AWP is placed on level ground. 

Remove any visible hazards that are in close proximity to the AWP and in the path that it will travel (both on the ground and in the air). 


	3. 
	Other workers or pedestrians entering work area
	Set-up work zone with caution tape to inhibit other workers or pedestrians from entering work area. 

Workers to wear the appropriate PPE (hard hat, steel toe boots, reflective vests, etc.) if they need to work in closer proximity to the AWP. 


	
	Slips from oil/fuel spills
	Ensure no fluids are leaking onto the ground.

Have spill kits readily available.  Clean up spills in a timely manner. 

Workers wear proper footwear. 

	Conducting an Inspection of the AWP
	Pinch Points
	Be aware of pinch points and keep hands and body parts away. 

	
	Equipment failure
	Follow the manufacturer’s specifications regarding inspection of the AWP.  

Inspect all parts to the AWP for defects, damage, etc. prior to use. If the AWP does not pass inspection, notify your supervisor and tag equipment so no one else operates the equipment. 


	
	Release of stored energy
	Be aware of areas where energy could be unexpectedly released (i.e. hydraulics failing). 

	Operating an AWP
	Contact with overhead power lines
	Identify any power lines that may be overhead where the lift is stationed and the path that it will travel. 

Maintain a safe distance from overhead power lines (minimum set-back distance is 18 feet).  If a safe distance cannot be maintained, employer to contact owner of the utility company to obtain a permit/assurance in writing. 

Develop a site-specific emergency response plan to rescue a worker who has come in contact with overhead power lines.      


	
	Dropped objects. 
	Barricade area below where AWP will operate.  Workers on the ground to wear hard hat. 

Utilize tool lanyards. 

	
	Tip-Over
	Operate the AWP in accordance with the manufacturer’s instructions.  

Do not exceed the weight limits of the AWP. 

Do not move the AWP in a raised position except to make minor adjustments.  If the AWP needs to be moved to a different location, lower the lift and proceed to move it. 

Develop a site-specific emergency response plan to rescue a worker if the AWP tips. 


	
	Contact with overhead structures
	De-energize (i.e. LO/TO) any electrical components that are overhead (i.e. fans, lighting, etc.).

Look up prior to raising the lift. Be aware of the path that the lift will be required to travel. 

All workers on an AWP to wear hard hats. 

Be aware of any trees, overhanging branches, or other structures. 

Develop a site-specific emergency response plan to rescue a worker who has come in contact with overhead structures. 


	
	Falling out of AWP
	Wear a fall arrest system (harness and lanyard) when using the AWP. 



Connect to the designated anchor points within the AWP. Do not connect to the guard rails (unless directed by the manufacturer). 

Do not use additional platforms or equipment to gain access to areas that the AWP cannot reach.

Maintain firm footing and do not overreach outside of the lift.  Stay within the guardrails at all time. 

Do not stand/climb on guard rails. 

Close gate/chain and ensure that it is in a locked position. 

Develop a site-specific emergency response plan to rescue a worker who has fallen out of an AWP. 

	
	Poor weather conditions (wind, rain, snow, etc.)
	Do not operate lift if the wind speeds exceed those outlined by the manufacturer.  

Do not operate in close proximity to power lines.  Remember that electricity can arc/jump and does not need to come in contact with the AWP. 

Inspect the AWP to ensure that it can be operated in adverse weather (i.e. snow). 

	
	Traffic and other machinery
	Be aware of traffic conditions on and near the site.  Use a spotter. 

Avoid coming in close proximity to other machinery on site. 

Make sure flashing lights and audible beepers are in good working order. 

	
	Ground Conditions
	Inspect ground conditions in the site area. Check to see if ground conditions have been affected by excavations, trenches, holes, or rocks. 

If the AWP has outriggers/stabilizers, use them to spread the load over a larger area.  Extend the outriggers to stabilize the machine and make level.  

	
	Exposure to exhaust fumes
	If operating a gas powered AWP, operate in a well-ventilated area. 

Turn off when working in enclosed work areas to prevent accumulation of exhaust fumes. 

Conduct regular maintenance on AWP. 

	
	Fire
	Have a fire extinguisher readily available on the AWP.  Review the SWP for operation of an fire extinguisher. 

Store flammable materials away from any source of ignition. 

	Other Hazards/Considerations:

	
	

	
	
	

	
	
	

	
	
	

	

	



