	JOB SAFETY ANALYSIS (JSA) FORM

	
Date:                                                                                       Location: ______________________________________________________

Job Being Performed:  Setting up an extension ladder and… _______________________________________________


	Sequence of Events / Work Activity
	Potential Accidents or Hazards
	Preventative / Control Measures

	1. Gather tools and equipment for task (including ladder)
	1.0 Awkward positioning causing strains or musculoskeletal injury (MSI)
1.1 Uneven ground causing slip, trip or fall 
1.2 Weather conditions (ie. Wind, rain, temperatures)
1.3 Other workers or pedestrians entering work area
	1.0.0 Use proper lifting techniques (ie. Lift with legs)
1.0.1 Have second worker aid with lifting
1.0.2 Use means of mechanical lifting if ladder cannot be safely lifted from storage location
1.0.3 Carry ladder to assist with set-up at work location (ie. Leg stabilizers towards rear so they can be set down and front lifted upwards)
1.1.0 Ensure path of travel is clear prior to obtaining ladder
1.1.1 Remove any visible hazards in walking path prior to moving ladder 
1.2.0 Verify wind speeds and ensure ladder can be safely set-up and used in current conditions
1.2.1 Be aware of potential electrical hazards that may increase due to rainy conditions
1.3.0 Set-up work zone with caution tape to inhibit other workers or pedestrians from entering work area




	Sequence of Events / Work Activity
	Potential Accidents or Hazards
	Preventative / Control Measures

	2. Stage and set-up ladder at work location
	2.0 Heavy lifting and/or straining while setting up ladder
2.1 Striking something while moving ladder to work location
2.2 Pinch points at extension ladder brackets and stops
2.3 Sharp edges along rails ladder legs
2.4 Electrical shock from ladder striking or near overhead powerlines
2.5 Ladder falling or unstable due to set-up
	2.0.0 Use proper lifting techniques (ie. Lift with legs)
2.0.1 Have second worker aid in lifting and set-up of ladder
2.0.2 Ensure worker(s) have a good handle on ladder (ie. Grip) prior to moving
2.1.0 Verify set-up area and use caution when turning to avoid striking something
2.2.0 Be aware of potential pinch points and keep hands away
2.3.0 Wear gloves to protect hands from any potential sharp edges
2.4.0 Perform survey of work area and identify if there are any overhead lines
2.4.1 If any overhead lines, ensure distances are maintained as required.
2.5.0 Ensure ladder legs are on firm, stable ground and are maintained level.
2.5.1 Secure ladder at top and bottom to ensure it will not “kick-out”
2.5.2 Set-up ladder using 4 to 1 ratio (for every 4’ up the ladder should be 1’ out)

	3. Climb ladder and commence work task
	3.0 Falling off ladder during work
3.1 …
3.2 …
	3.0.0 Maintain 3-point contact when ascending and descending ladder
3.0.1 Never over-reach when working on a ladder, move ladder as required.
3.0.2 Ensure workers keep center of gravity between ladder rails
3.1.0 …
3.2.0 …

	
	
	

	Other Hazards/Considerations:

	
Signing this hazard assessment form indicates you have reviewed and understood all hazards and controls to be put in place:

_______________________________________      __________________________________________     ___________________________________ 

_______________________________________      __________________________________________     ___________________________________

_______________________________________      __________________________________________     ___________________________________

Signature of supervisor: __________________________________________                                                      Date: ___________________________________



