	JOB SAFETY ANALYSIS (JSA)

	
Date:                                                                                       Location: ______________________________________________________

Job Being Performed:  Reviewing Slip, Trip and Fall Hazards in the Workplace


	Sequence of Events / Work Activity
	Potential Hazards
	Preventative / Control Measures

	 Examining ground conditions associated with working outside (Field Work, construction work prep, etc.).
	Uneven ground causing slip, trip, or fall (uneven concrete, uneven or loose ground, potholes, manhole coverings, sidewalks, curbs, loose rocks, stairways, walkways, etc.)
	Ensure path of travel is clear prior to starting task.

Remove any visible hazards in walking path prior to the start of work.

Identify uneven surfaces by highlighting with hi-visible spray paint or place signage in area (where practical).

Hold TBT daily with crew (where practical) to identify, mitigate or eliminate such hazards.

Develop or review existing safe work practices, and/or procedures for hazards involved with groundwork such as Trenching and excavation, construction work prep, etc.).

Inspect ground conditions in the site area. Check to see if ground conditions have been affected by excavations, trenches, holes, or rocks.

	1. 
	Wet / Slippery Surfaces or ground due to weather conditions or daily operations (ice, snow, rain fall, mud, etc.).
	Hold TBT daily with crew (where practical) to identify, mitigate or eliminate such hazards.

Ensure path of travel is clear prior to starting task.

Remove any visible hazards in walking path prior to the start of work. (Use ice controls such as salt or sand, shovel or have snow cleared, etc.).

Cautionary signage is available and placed in work areas that these conditions are a part of daily operations.

Inspect ground conditions in the site area. Check to see if ground conditions have been affected by excavations, trenches, holes, or rocks. 

	2. [bookmark: _Hlk95296373]
	Tools or objects improperly placed on ground
	Maintain good housekeeping practices by ensuring that all tools and equipment are cleaned up or moved into another area to eliminate trip and fall hazards.

Ensure cords are properly stored (coiled up or stored inside cord trays where practical).


	
	






Wet or dry containments spilled on surfaces (Oil/fuel spills, chemicals, etc.)







	Ensure good housekeeping practices are implemented (i.e. –surfaces or ground in cleaned up in a timely manner.

Workers all trained in WHMIS and understand how to read MSDS for proper cleanup of chemical spills, etc. 

Barricade or berm area that has chemical spill until it can be cleaned and adequately addressed.

Spill kits readily available.

Ensure spill is reported and all applicable parties are aware or have been informed.

Review (where applicable) safe work practices or procedures related to environmental spills, reporting, etc. 


	
	Falling off ladder when climbing up or down

	Maintain 3-point contact when ascending and descending ladder.

Never over-reach when working on a ladder, move ladder as required.

Ensure workers keep center of gravity between ladder rails.

Inspect the ladder and ground conditions before use.

Check weather conditions prior to completion of worker and where possible use ladder when conditions are dry.
Workers to wear nonslip footwear.

	Examine floor/surface conditions before the start of work (Working Inside a facility, office, on a shop floor, entryways, stairways, walkways, etc.).
	Uneven ground causing slip, trip, or fall (uneven concrete, loose or soft ground conditions, raised manholes, potholes, stairways, walkways, etc.)
	Good communication with crew via toolbox talk to discuss work and any hazards related to the task and work area.

Ensure path of travel is clear prior to starting task.

Remove any visible hazards in walking path prior to the start of work.

Identify uneven surfaces by highlighted with hi-visible spray paint or place signage in area (where practical).

Ensure workers are trained in Standard First Aid/CPR.

Develop a site-specific emergency response plan to capture various slip and fall scenarios.

	
	Wet or Slippery Surfaces due to weather conditions or a part of daily operations (i.e., walkways, stairways, shop floors, entrances, etc.).
	Ensure good housekeeping practices are implemented (i.e. – floors are mopped to keep as dry as possible)

Cautionary signage such as: “Wet Floor” or “Slippery When Wet” are available and placed in work areas that these conditions are a part of daily operations.

Consider using a non-Slip flooring/, a flooring paint that has a course texture, or add mats to areas that have high potential for slips, trips and falls. 

Ensure that that there is floor drainage and that it is not obstructed.

Barricade area that has slippery surfaces until hazard can be addressed (cleaned up, etc.).

Workers trained in Standard First Aid/CPR

Workers to wear nonslip footwear.


	
	











Wet or dry containments spilled on surfaces (Oil/fuel spills, chemicals, etc.)












	Ensure good housekeeping practices are implemented (i.e. –surfaces are cleaned up or kept as dry as possible).

Workers all trained in WHMIS and understand how to read MSDS for proper cleanup of chemical spills.

Barricade or berm area that has chemical spill until it can be cleaned and adequately addressed.

Cautionary signage such as: “Wet Floor” or “Slippery When Wet” are available and placed in work areas that these conditions are a part of daily operations.

Consider using a non-Slip flooring, a flooring paint that has a course texture, or add mats to areas that have high potential for slips, trips and falls. 

Ensure that that there is floor drainage and that it is not obstructed.

Workers to wear nonslip footwear.
Spill kits readily available.


	
	Tools or objects improperly placed on floor
	Maintain good housekeeping practices by ensuring that all tools and equipment are cleaned up or moved into another area to eliminate trip and fall hazards.

Ensure cords are properly stored (coiled up or stored inside cord trays where practical).


	
	Falling off ladder when climbing up or down

	Maintain 3-point contact when ascending and descending ladder.

Never over-reach when working on a ladder, move ladder as required.

Ensure workers keep center of gravity between ladder rails.

Ensure that ladder is placed on even and steady ground/surface.

Workers to wear nonslip footwear.


	
	Tripping or falling on mezzanine or raised areas
	Maintain 3 points of contact when ascending and descending mezzanine or raised areas (holding handrails).

Ensure good housekeeping practices are implemented (i.e., surfaces are cleaned up or kept as dry as possible).

Cautionary signage such as: “Wet Floor” or “Slippery When Wet” are available and placed in work areas (where practical). Barricade area 
that has slippery surfaces until hazard can be addressed (cleaned up, etc.).

Develop a site-specific emergency response plan to capture various slip and fall scenarios.

Consider using a non-Slip flooring/, a flooring paint that has a course texture, or add mats to areas that have high potential for slips, trips and falls. 

Workers trained in Standard First Aid/CPR

Workers to wear nonslip footwear


	Ascending or descending from high to low or low to high areas. (i.e., Working on heavy equipment, Flat Bed Trucks, vehicles, ladders, mezzanines, etc.).
	Fall causing injury to worker while ascending/descending heavy equipment, fall bed truck, vehicle, etc.
	Develop a site-specific emergency response plan to capture various slip and fall scenarios.

	
	Uneven ground causing slip, trip, or fall (loose or soft ground, uneven concrete, 
	Ensure path of travel is clear prior to starting task.

Identify uneven surfaces by highlighting with hi-visible spray paint or place signage in area (where practical).

Hold TBT daily with crew (where practical) to identify, mitigate or eliminate such hazards.

Develop or review existing safe work practices, procedures for hazards involved with groundwork.


	Other Hazards/Considerations:







	
Signing this hazard assessment form indicates you have reviewed and understood all hazards and controls to be put in place:

______________________________________      __________________________________________     ___________________________________ 

______________________________________      __________________________________________     ___________________________________

______________________________________      __________________________________________     ___________________________________

Signature of supervisor: ________________________________________                                           Date: ___________________________________




