TRAVEL OVER AND WORK ON WATER AND ICE
When working on or about water the following conditions must be met:
· Lifebuoys measuring 76.20 centimeters diameter shall be provided during working hours on all fixed and floating structures where workers are employed on or about the water.
· Lifebuoys shall be fitted with not less than 15.24 meters of 9.52 millimeters diameter manila rope or other material of equal strength and the lifebuoys shall be placed in conspicuously marked locations spaced at intervals not exceeding 76.20 meters.
· Lifebuoys must meet the requirements of standards acceptable to the Canadian Coast Guard.
· Floats or rafts used as work stages with staging erected on them shall be constructed and used so that workers are not endangered by instability or excessive movement of the equipment.
· When workers are employed on floating equipment exposed to the hazards of weather or the movement of water traffic, the equipment shall be provided with a warning or signaling device for use in case of distress, fog or other hazardous or emergency circumstances.
· Whenever workers are employed on floating equipment, a boat ready for immediate use shall be available for rescue or escape.
As per s. 27 of the OHS regulations, where a worker is to travel over or work on ice and the water beneath the ice is more than one meter deep at any point, this company will ensure the ice supports the load to be placed on it. The ice shall be checked before the work begins, and as often during the work as necessary to ensure the safety of the workers.
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