ADHESIVES
· Many adhesives are toxic. Care must be taken to avoid breathing the vapours.

· Ensure ventilation is adequate when using adhesives. Local exhaust ventilation is recommended.
·  Many adhesives are flammable. Ensure vapours are kept away from sparks, flames and sources of ignition. Do not weld or cut on or near adhesive containers.

· Solvent vapours are heavier than air and may travel along the ground or floor, or be moved by ventilation and ignited by heat, pilot lights, other flames and ignition sources at locations distant from the material handling point. Nearby welding or cutting torches can explosively ignite adhesive vapours.

· Keep container closed to contain vapours. Emptied containers retain vapours from product residue.

· Avoid contact with eyes, skin and clothing.
· Wash thoroughly after handling.
· Become familiar with the M/SDS before using an adhesive.

· Observe all labelled precautions until containers are cleaned or disposed of. 
· Wear appropriate personal protective equipment such as rubber gloves to prevent skin contact, safety glasses to reduce potential for eye contact and organic vapour respirators when airborne exposure limits are exceeded. 
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