
CHAIN SAWS
· Chain saws must comply with CSA Standards Z62.1, Chain Saws.

· Workers must be trained in the safe operation of the chain saw.
· The correct method of starting, holding, carrying, storing, and using the saw, as directed by the manufacturer, must be followed.

· A worker operating a chain saw shall wear a leg protective device with a label permanently affixed to the outer surface of the device indicating the standard it meets.
· A chain saw shall have a chain brake that activates automatically upon kickback regardless of the position of the power head or operator's hands. 
· The chain must be sharp, have the correct tension, and be adequately lubricated.
· The chain saw must not be used for cutting above shoulder height.
· A chain saw chain shall be stopped before the saw operator moves from cut to cut, unless the next cut is in the immediate area and the saw operator can safely move to the next cutting position.
· When carrying/transporting a chain saw the bar guard must be in place, the chain bar must be toward the back and the motor must be shut off.

· Fuelling of the saw must be done in a well ventilated area and not while the saw is running or hot.

· An approved safety container must be used to contain the fuel used along with a proper spout or funnel for pouring.
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