GRINDING
· Check the tool rest for the correct distance from the abrasive wheel, maximum 1/8" or 3 mm.

· Replace the grindstone when adjustment of the rest cannot provide 1/8" or 3 mm clearance.

· If the wheel has been ground to an angle or grooved, reface the wheel with the appropriate surfacing tool.

· Protect your eyes with goggles or a face shield at all times when grinding.

· Each time a grinding wheel is mounted, the maximum approved speed stamped on the wheel bladder should be checked against the shaft rotation speed of the machine to ensure the safe peripheral speed is not exceeded.  A grinding wheel must not be operated at peripheral speed exceeding the manufacturer's recommendation.

· The flanges supporting the grinding wheel should be a maximum of 1/3 the diameter of the wheel, and must fit the shaft rotating speed according to the manufacturer's recommendation.

· Bench grinders are designed for peripheral grinding.  Do not grind on the side of the wheel.

· Do not stand directly in front of grinding wheel when it is first started.
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