
HAND-HELD POWER CIRCULAR SAWS
· Approved safety equipment such as safety glasses or a face shield are to be worn.

· Where harmful vapours or dusts are created, approved breathing protection is to be used.

· The proper sharp blade designed for the work to be done must be selected and used.

· The power supply must be disconnected before making any adjustments to the saw or changing the blade.

· Before the saw is set down be sure the retracting guard has fully returned to its down position.

· Both hands must be used to hold the saw while ripping.

· Maintenance is to be done according to the manufacturer's specifications.

· Ensure all cords are clear of the cutting area before starting to cut.

· Before cutting, check the stock for foreign objects or any other obstruction which could cause the saw to "kick back".

· When ripping, make sure the stock is held securely in place.  Use a wedge to keep the stock from closing and causing the saw to bind.
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