
OPERATION OF AIR TOOLS
· Review the manufacturer's instructions before using a tool.
· Wear safety glasses or goggles, or a face shield (with safety glasses or goggles), and, where necessary, safety shoes or boots and hearing protection. 
· Post warning signs where pneumatic tools are used. Set up screens or shields in areas where nearby workers may be exposed to flying fragments, chips, dust, and excessive noise. 
· Ensure that the compressed air supplied to the tool is clean and dry. Dust, moisture, and corrosive fumes can damage a tool. An in-line regulator filter and lubricator increases tool life. 
· Keep tools clean and lubricated, and maintain them according to the manufacturers' instructions. 
· Use only the attachments that the manufacturer recommends for the tools you are using. 
· Be careful to prevent hands, feet, or body from injury in case the machine slips or the tool breaks. 
· Reduce physical fatigue by supporting heavy tools with a counter-balance wherever possible.
· Do not use an air tool for any purpose other than what it is intended for.
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