USE OF PROPANE
· All installations and use of this product on the job-site must comply with the provincial legislation set out for its safe use. 
· Nylon slings must be used in a "choker" fashion when loading, off-loading or lifting propane tanks.

· "Lifting lugs" provided on tanks are not to be used.  Slings are to be wrapped around the shell of the tank.

· Tank valves and regulators are to be removed from the tank prior to any movement of the tank.

· Crane hooks shall be equipped with a “safety latch".

· All trucks, cranes or equipment used to handle propane tanks must be equipped with a fire extinguisher appropriate for the size and type of tank being handled,

· Except in an emergency, any movement or repositioning of tanks shall be performed by a competent worker.

· Tanks are not to be heated to increase flow.

· When in use, propane bottles are to be securely held in an upright position.

· Tanks are not to be hooked up and used without proper regulators.
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