


	FALL PROTECTION EQUIPMENT INSPECTION FORM

Serial/Equipment #:____________________Inspected By:_______________________


	Components

	Accepted/
Rejected
	Comments

	Harness Inspection  Webbing
Watch for frayed edges, broken fibers, pulled stitches, cuts, burns, and chemical damage.
	Accepted

Rejected
	

	“D” Rings/Back Pads
Check “D” rings for distortion, cracks, breaks, and rough or sharp edges.  The “D” ring should pivot freely.  “D” ring back pads should also be inspected for damage.
	Accepted

Rejected
	

	Attachment of Buckles
Note any unusual wear, frayed or cut fiber, or distortion of the buckles.
	Accepted
Rejected
	

	Tongue/Grommet
The tongue receives heavy wear from repeated buckling and unbuckling.  Inspect for loose, distorted or broken grommets.  The webbing should not have any additional punched holes.
	
Accepted

Rejected
	

	Other: Tongue Buckle
Buckle tongues should be free of distortion in shape and motion.  They should overlap the buckle frame and move freely back and forth in their socket.  The roller should turn freely on the frame.  Check for distortion or sharp edges.
	
Accepted

Rejected
	

	Friction and Mating Buckles
Inspect the buckle for distortion.  The outer bars and center bars must be straight.  Pay special attention to corners and attachment points of the center bar.
	
Accepted

Rejected
	

	Lanyard Inspection Hardware
Snaps: Inspect closely for hook and eye distortions, cracks, corrosion, or pitted surfaces.  The keeper (latch) should seat into the nose without binding and should not be distorted or obstructed.  The keeper spring should exert sufficient force to firmly close the keeper.  Keeper locks must prevent the keeper from opening when the keeper closes.
	
Accepted

Rejected

	

	Web Lanyard
While bending the webbing over a curved surface such as a pipe, observe each side of the webbed lanyard.  This will reveal any cuts or breaks.  Examine the webbing for swelling, discoloration, cracks, or burns.  Observe closely for any breaks in the stitching.
	
Accepted

Rejected
	

	Rope Lanyard
Rotation of the rope lanyard while inspecting from end to end will bring to light any fuzzy, worn, broken or cut fibers.  Weakened areas from extreme loads will appear as a noticeable change from the original diameter.  The rope diameter should be uniform throughout, following a short break-in period.  Make sure the rope has no knots tied in it.  Knots can reduce the strength of the rope by up to 60%.
	
Accepted

Rejected

	

	Shock-absorbing Lanyard
Shock-absorbing lanyards should be examined as a web lanyard.  However, also look for signs of deployment.  If the lanyard shows signs of having been put under load (e.g. torn out stitching), remove it from service.
	
Accepted

Rejected
	

	
Date Inspected:_________________________________________
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