
AERIAL PLATFORMS
· Read and follow manufacturer operating instructions.
· Ensure correct aerial platform is utilized.

· Ensure workers are properly trained in the operation of the aerial platform.
· Perform inspections of the platform as per manufactures recommendations.
· Ensure ground is firm and level.
· Be aware of power line proximity.
· Do not overload the machine at any time.
· Wear a safety harness attached to the designated anchor point when operating any aerial platform.
· Get on and off the platform when it is in lowered position.
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