DUMP TRUCK LOADING AND HAULING

· A PRE-OPERATION CHECKLIST is required before operating the equipment. 

· Prior to loading material into a dump truck the loader operator must signal that she/he is ready to start loading (example beeping the  horn) 

· Prior to hauling the material the loader operator must signal that the loading process is finished and the dump truck driver is cleared to leave. 

· DO NOT load over the truck capacity.  

· When hauling on public roads, ensure that load covers are deployed and loose materials on the edge of the dump box and around the tailgate have been removed. 

· Follow all traffic signs and drive at or below the posted speed limit.

· Be courteous to other drivers and pedestrians.

· Make sure heavy equipment mirrors are adjusted and free from debris that may obstruct the operators view.

· Turn on hazard lights when the dump truck is operating at reduced speed to warn other drivers.

· If dump truck is operating at reduced speed on a public road, periodically check for buildup of traffic behind truck.

· Pull over and allow traffic to pass. ONLY if it is SAFE to do so.
