STORAGE AND HANDLING OF MATERIALS


· Follow instructions on all packaging labels, i.e., Fragile, This Side Up as well as any
hazardous information.

· Never store materials in such a manner to block walkways or exits.

· Do not stack material high enough that it is unstable.

· Store material in dry locations.

· When Data Information Sheets are applicable, make copies available in the stored area.

· When material is returned to the warehouse, check with your supervisor if you are unsure
of the proper storage area.

· When possible, leave all labels facing forward.

· When transporting goods by vehicles, follow all Motor Vehicle regulations regarding
overhangs from tailgates and securing cargo.

· If hoisting is required, follow the proper procedures.

· When storing pipe and other cylindrical objects above grade level brace the material to
	prevent it from rolling to an unwanted area.
