
Ladder Inspection Checklist
	Company Name:
	[bookmark: Text1]     
	[bookmark: Check1]|_|  Pre Shift   
[bookmark: Check2]|_|  Hourly
[bookmark: Check3]|_|  End Of Day

	Location:
	[bookmark: Text2]     
	

	Employee in Charge
	Immediate Supervisor
	Date YYYY/MM/DD
	Time   □  A.M.
          □  P.M.

	[bookmark: Text3]     
	[bookmark: Text4]     
	[bookmark: Text5]     
	[bookmark: Text6]     

	Sub-Contractor
	Type of Operation
	Crew Size

	[bookmark: Text7]     
	[bookmark: Text8]     
	[bookmark: Text9]     

	· Step Ladder Extension
· Extension Ladder
Serial No.      
	NOTES
     


[image: ]


	
 Inspect Unit Carefully 

	Steps, Rungs, Uprights & Braces
	YES
	NO
	Comments

	Loose or missing steps
	|_|
	|_|
	     

	Loose Fasteners or other metal parts 
	|_|
	|_|
	     

	Cracked, Broken, Split or Worn
	|_|
	|_|
	     

	Slivered 
	|_|
	|_|
	     

	Damaged/worn non-slip bases 
	|_|
	|_|
	     

	Sharp edges on rails or rungs
	|_|
	|_|
	     

	Missing or illegible identification labels
	|_|
	|_|
	     



	Hinges
	YES
	NO
	Comments

	Loose Hinge
	|_|
	|_|
	     

	Loose/Bent Spreader
	|_|
	|_|
	     

	Spreader stop broken  
	|_|
	|_|
	     

	Rust
	|_|
	|_|
	     

	Moveable parts operate freely 
	|_|
	|_|
	     



	Locks & Rope
	YES
	NO
	Comments

	Loose, broken, or missing lock
	|_|
	|_|
	     

	Improperly seated when extended 
	|_|
	|_|
	     

	Worn or rotted rope 
	|_|
	|_|
	     




	Inspection Completed By:
	     
	Signature:
	

	Reviewed By:
	     
	Signature:
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