
LANYARD INSPECTION

Model: ______________________	   	Serial # ______________________		Date of Manufacture:  ___________________

Type of Lanyard:
  Energy/Shock Absorbing 		  Flat Web		  Tubular Energy Absorbing		  Tie-Back/Wrap-Back      	
  Double- Legged 			  Cable		  Rope					  Chain Positioning		
  Other: __________________________________________________________________________
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Name of Inspector __________________________________

Signature of Inspector _____________________________

Date _____________
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DEFINITION OF TERMS

Deterioration - Eaten or worn away by chemicals

Pitting - A small indentation in a surface

Nicks - A shallow notch, cut, or indentation on an edge or surface
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