


	Work Activity
	Related Activity
	 (
Comprehensive Hazard Report: Garbage Services
)Hazards
	Risk Ranking
Risk = Severity+Probability+Frequency
	Controls

	
	
	
	S
	P
	F
	RR
	

	Waste Equipment Operation
	Completing a Circle Check
	Slips Trips and Falls

	1
	1
	2
	4
	· Good House Keeping
· snow removal and de-icing agents

	
	
	Being Struck by Other Equipment

	4
	1
	2
	7
	· Lighting
·  PPE

	
	
	Exposure to Exhaust Fumes 


	2
	1
	1
	4
	· Idle only in well ventilated areas 
· use ventilation system if vehicle is in the shop

	
	Operating
	Inexperienced Operator
	3
	2
	1
	6
	· Licensed Drivers
· In house training


	
	
	Traffic on Public Roadways
	1
	3
	3
	7
	· Use of Spotters to stop traffic if required
·  Amber Strobe lights /emergency flashers and work lights
· Audible Back Up beepers


	

	


	
Bystanders / Construction Crews
	4
	2
	2
	8
	· PPE
· Spotters when required
· Amber Strobe lights /emergency flashers and work lights
· Audible Back Up beepers

	
	
	Sprains/Strains climbing in and out

	3
	3
	3
	9
	· SWP Garbage Collection


	
	


	Road and Ground Conditions

	3
	2
	2
	7
	· Trained Drivers
· SWP Delivering/Removing Containers
· Use de-icing agents’
· Adjust routing to accommodate slippery or impassible roadways
· Use Planks to protect Driveways 


	
	
	Weather

	1
	3
	2
	6
	· PPE
· Extra Clothes i.e. Gloves
· Sunblock
· Water


	
	


	Mechanical Failure

	1
	1
	1
	3
	· PPE
· Flare Kits
· Fire Extinguisher
· Communication / Emergency Contact Numbers


	
	
	Oversized/Overweight Loads

	1
	1
	1
	3
	· SWP picking up containers
· Load must be secured before we travel
· Remove Material if required

	
	Backing Up
	Striking Object or Individual
	4
	3
	3
	10
	· Use Spotter when visibility is compromised
· Audible Back up Beeper
· Back Up Cameras




	
	
	Overhead Power Lines
	4
	1
	1
	6
	· SWP Power Line Hazards
· Permit from Utility if Closer than 18 Ft
· Power Line Hazard Training
· Emergency Response Plan for Accidental Contact
· First Aid
· Fire Extinguisher
· Use of a Spotter when required

	
	
	
	
	
	
	
	· 

	
	
Container Deliveries Removals


	Drop Offs / Deliveries
	4
	2
	2
	8
	· Trained Operators
· SWP Container Delivery
· Spotters to stop traffic
· PPE


	
	
	Pick Ups / Removals
	4
	2
	2
	8
	· Trained Operators
· SWP Container Pick Up
· Spotters to stop traffic
· PPE

	
	
	Poor Ground Conditions
	4
	2
	2
	8
	· Informal Hazard Assessment
· Only Park and operate on firm solid level ground
· Beware of soft narrow shoulders
· Beware of excavated area’s

	
	Unloading
	Overhead Power Line Contact
	4
	1
	1
	6
	· SWP Unloading Waste Equipment Roll Off, Compactor Trucks 


	
	
	Blowing and Falling Debris
	2
	2
	2
	6
	· PPE
· Access Load before opening door
· Open One Door at a time and stand away from the pinch points

	
	
	Cuts, Boot Punctures
	2
	2
	2
	6
	· PPE
· Aware of Surroundings
· Vaccinations  

	
	
	Being Struck by other Equipment
	4
	1
	2
	7
	· PPE
· Follow Site Rules

	
	
	Roll Over's
	4
	1
	1
	6
	· Check to ensure load is balanced
· Ground must be solid and level
· Remain inside cab while dumping

	
	Tarping Loads
	Falling Materials
	2
	2
	2
	6
	· PPE
· Inspect load at ground level before picking up
· Remove all hanging debris

	
	
	Overhead Obstructions
	3
	2
	2
	7
	· PPE
· Hazard Assessment ie roof eves, wires

	
	Loading: Residential Collection
	Slip Trips and Falls
	3
	3
	3
	9
	· PPE
· Situational Awareness (Broken Curb, ice, catch basins, sand covered asphalt etc)
· SWP Residential Garbage Collection

	
	
	Needle Pricks / Cuts and Lacerations
	4
	2
	3
	9
	· PPE
· Vaccinations
· SWP Needle Pricks, Residential Garbage Collection

	
	
	Flying Debris
	2
	1
	1
	4
	· PPE
· Training

	
	Compacting Garbage in Truck
	Pinch Points
	4
	2
	1
	7
	· Machine Guarding
· Training
· Labels
· Lock out Procedures

	
	
	MSI, Repetitive Strain 
	3
	3
	3
	9
	· Job Procedure Residential 
· Garbage Collection

	
	Fueling
	Spills
	1
	1
	1
	3
	· Spill Kits
· PPE

	
	
	Fire/Explosions
	1
	1
	1
	3
	· Fire Extinguishers
· Emergency Contact Numbers

	
	
	Vapors/Gas exposure
	1
	1
	1
	3
	· Well ventilated areas














Comprehensive Hazard Assessment
Risk Ranking
Severity
+0 No Injury
+1 Minor Injury requiring first aid 
+2 Medical treatment with no lost time beyond the day of injury and minor property damage ($500 or less)
+3 Lost Time Injury or significant property damage (greater than $500 but less than $5000)
+4 Permanent Disability/Fatality(ies) or major property damage (greater than $5000)

Probability

	+1 Exposure to the uncontrolled hazard is unlikely to occur
	+2 Exposure to the uncontrolled hazard could occur
	+3 Exposure to the uncontrolled hazard will occur

Frequency
	
	Number of Persons Exposed
	Number of times persons may be exposed to or have contact with the hazard.

	
	Less than daily
	Few times a day
	Many time a day

	Few
	+1
	+1
	+2

	Moderate
	+1
	+2
	+3

	Many
	+2
	+2
	+3



Risk = Severity + Probability + Frequency   

Low Risk 0-2           Medium Risk 3-5           High Risk 6-10
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