HAZARD CONTROL SIGNAGE
· Work sites should have appropriate and adequate signage to identify site hazards in place prior to the commencement of any work process.

· Ensure signage is in good condition, clean, legible and suited to the purpose.
· Ensure traffic control signage is to be of accepted standards.
· Ensure signage is secured.
· Routinely inspect signage for placement, cleanliness and physical damage.
· Ensure road traffic control signage is covered when no activity is present.
· Ensure you are fully trained to erect road traffic signage.
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