USE OF METAL SCAFFOLDS
· Ensure the scaffold you intend to use is the correct one for the job.
· Ensure the scaffold will be erected by a competent worker in accordance with the manufacturer’s instructions.
· Ensure legislative requirements are met, including the provisions for scaffold planks. 
· The location in which the scaffold is to be constructed must be level or capable of presenting secure footing by use of mudsills or some other device.
· Safe access and egress to both the scaffold and the general work area must be provided.
· Ensure levelling adjustment screws have not been over extended.
· All guardrails must be in place.
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