USE OF PORTABLE GRINDERS
· Familiarize yourself with the grinder operation before commencing work.

· Ensure proper guards are in place and that safety glasses, face shields, gloves and safety boots are worn when using portable grinders.

· Never exceed the maximum wheel speed (every wheel is marked).  Check the speed marked on the wheel and compare it to the speed on the grinder.

· When mounting the wheels, check them for cracks and defects, ensure that the mounting flanges are clean and the mounting blotters are used.  Do not over tighten the mounting nut.

· Before grinding, run newly mounted wheels at operating speed to check for vibrations.

· Do not use grinders near flammable materials.

· Never use the grinder for jobs for which it is not designed, such as cutting.
· Proper storage, proper use, and proper maintenance of wheels must be observed.
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