SPRAY PAINTING

· Ensure appropriate training and familiarity with safe work procedures.

· Follow manufacturers recommendations.

· Ensure all sources of ignition are eliminated.

· Ensure equipment is grounded.

· Ensure area is ventilated.

· Do not smoke around spray painting operations.

· Ensure warning signs are in place.

· Practice good housekeeping.

· Ensure all appropriate personal protective equipment is worn.
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